PATEL ROAD PUMP HOUSE SUMMARY

1. PARAPET WALL IS MISSING MOSTLY
2. COMPONENT MISSING IN SOME PLACES
3. PUMP AND PIPE SIZE IS NOT MATCHING WITH RCP
4. PIPE VALVE IS MISSING AND SIZE IS NOT MATCHING
5. SUNSHADE IS NOT MATCHING WITH RCP IN ONE PART OF BUILDLING
6. PIPE SUPPORT IS MISSING IN ALL AREA
7. PIPE POSITION NOT MATCHING WITH RCP
8. STEEL MEMBER IS MISSING
9. WALL TOP OFFSET HEIGHT IS MISMATCHING
10. WINDOW OPENING IS MISSING
11. CHECK GATE OPENING HEIGHT
12. OVERHEAD CRANE MISSING
13. RAINWATER GUTTER IS MISSING
14. JOINGEOMETRY ISSUE